#### Controller Information

The Controller Information area displays the controller discovered by PC-DMIS during online execution. This section shows four display boxes with this information:

- Controller drop-down list: Select your machine model for interfaces that support multiple machine models. For example, the Metronics interface would have “TESA VISIO 300 Manual”, “TESA VISIO 300 DCC” and “Custom” types. This option MUST be set in order to configure machine configuration settings correctly for the target machine. For interfaces that only support one type of machine, the option will have been automatically preselected for you.

- PC-DMIS connectivity: Displays the supported version of the Hardware Abstraction Layer (HAL) interface for this version of PC-DMIS supports. The HAL version should be the same for PC-DMIS, MSI and HSI. A warning will be given if differences are encountered.

- MSI (Multi-Sensor Interface) connectivity: Displays the supported version of the HAL interface for this MSI.

- HSI (Hardware Specific Interface): Displays the HSI used during execution. This component controls the specific hardware device.

- CMMI (Coordinate Measuring Machine Interface): Displays the name of the CMMI interface to be used. Click Setup... to open the Machine Interface Setup options for the CMMI controller (e.g. B&S LEITZ).

You should provide this information to your PC-DMIS technical support group when you report problems.