### A Note on Executing a Vision Part Program

When you are executing your part program there are steps that can be taken that will cause a feature to be in tolerance (PASS) or out of tolerance (FAIL). This is done by clicking Continue in the Execution Mode Option dialog box to PASS the feature or by clicking Skip to FAIL the feature.

- If you PASS a feature, the MEAS values for the CENTROID are set to the THEO values.

- If you FAIL a feature, the MEAS values for the CENTROID are set to the THEO values + 100mm in the probe vector direction (usually Z). The feature will show in the Graphics Display window as floating above the part. However, if looking straight down in the Graphics Display window, the feature will appear to be drawn correctly.

So, if you have a dimension on the position of the feature, it will be in tolerance or out of tolerance, depending on whether you clicked Continue or Skip.