## Step 4: Install PC-DMIS

The following steps run you through a typical installation. Your installation screens may differ if you are running a different version of PC-DMIS. In addition, your USB portlock might be configured with different options.

1. Ensure your USB portlock is connected to your machine.

2. Locate the PC-DMIS installation file, setup.exe, on your installation media; or if you downloaded it, open the directory containing the downloaded file.

3. Double-click setup.exe file to begin the installation process. If presented with a security warning, click Run.

4. The files are extracted to a temporary directory:

5. The Choose License Type screen appears.

Click on one of the following license types:

- HASP - If you have a physical USB portlock key, click this item. This is selected by default.

- LMS (Software) License - If you have been issued a software license (called an entitlement ID), or if you will connect to a local license server, click this item.

Click Next to proceed.

6. If you chose Hasp, ignore this step, and proceed to step 7. If you chose, LMS (Software License), and it cannot find a valid license on your system, you need to fill out the LMS License Setup dialog box:

Fill out the LMS License Setup screen as needed:

- Use Entitlement ID - If you have an Entitlement ID, select this item, and then type the ID you were issued in the box.

- URL to FNO Services - This should point to the URL that verifies your license. Ensure it has this URL:
  https://licensing.wilcoxassoc.com/flexnet/services

- Proxy Information - You only need to fill this out if you are on a network where a proxy server is needed to reach the Internet. Contact your IT department to get this information and then fill in the server host, username and password.

- Use License Server(s) - If you are using a local license server, select this item, and then type your license server name. The format of this line of text should be <portnumber>@<servername>, where <portnumber> is the TCP port number for the license server and <servername> is the name of the server. The default TCP port number is 27000 and is used automatically if no specific port number is identified. For example, these mean the same thing:

@server1

27000@server1

You can also specify multiple license servers. These are separated by semicolons. For example, suppose you have three license servers called licenseserver1, licenseserver2, and licenseserver3 all using the default TCP port. You can specify all of them in a single line of text, like this:

@licenseserver1;@licenseserver2;@licenseserver3

Click Next to proceed. The install software connects to the Internet and activates your license and installs the FLEXnet Licensing Service required to use LMS licenses.

7. The main setup interface then appears. Click the Next to start the installation.

8. The license agreement then appears. Read and accept the license agreement, and then click Next.

9. Choose a setup type from the Choose Setup Type screen:

- Typical: This option installs the program files to the default installation location: C:\Program Files\WAI\PC-DMIS 2013\

- Custom: This option lets you specify what components to install as well as customize the installation location. A screen similar to the one below opens:

Overview of Customize Installed Features

By default, all program components are selected to be included in the installation. You can use the tree view to customize when or if these features are installed. To do this, click small drop-down icon next to the component to exclude. You'll see a drop down list.

Choose the desired option:

- Will be installed on local hard drive - The selected feature is installed to the hard drive on your computer.

- Entire feature will be installed on local hard drive - The entire feature is installed to the hard drive on the computer. This means sub-features of the selected feature are also installed.

- Will be installed to run from network - This option is currently unsupported. Installs the selected feature on a network share.

- Entire feature will be installed to run from network - This option is currently unsupported. Installs the entire component to network share. This means sub-features of the selected feature are also installed.

- Feature will be installed when required - The feature will only be installed if required during the installation process. Some files are informational and are not required for the application to run. These may include documentation or other files.

- Entire feature will be unavailable - This excludes the component from installation.

Customize Installation Location

By default, the program installs to this location "C:\Program Files\WAI\" under the "PC-DMIS 2013" directory. To change the default location, click the Browse button and navigate to the directory on your computer you want to hold the program files. When you click OK, the Location box changes to show the selected location.

Click Reset at any time to reset the items to the default selection.

Click Next when finished customizing the install.

10. Once the installation has all the information it needs, the Ready to Install screen opens:

11. Click Install to proceed with the main installation.

12. Once installation finishes, this final screen appears:

- Launch PC-DMIS after the install finishes - Mark this check box if you want to launch the application once you click Finish.

- Display Release Notes - Mark this check box if you want to see a simple PDF file showing what's new or changed in this release once you click Finish.

13. Click Finish to close the installation program. PC-DMIS is now installed.