core

### Mora Interface

The Mora interface is used with Mora CNC machines. This interface just requires a single RS232 comm port; no machine parameter file is needed from the original system.

Before you start PC-DMIS, rename the mora.dll to interfac.dll.

The Machine Options dialog box (Edit | Preferences | Machine Interface Setup) has these tabs for the Mora interface:

Comm tab

See the "Setting the Communication Protocol" topic. Default value is Comm Port 1, 9600 Baud, No parity, 8 data bits, and 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).

You can access the MIIM help file from this link: .