laser

#### Initial Touch Vector (InitVec)

The values that are displayed in the Initial Touch Vector row indicate the vector PC-DMIS will use to take the first touch in the scanning process.

To edit the I, J, K Initial Touch vector:

1. Double-click on InitVect in the vector column to open the Edit Scan Item dialog box.

2. Change the values.

3. Click the OK button to accept the changes and close the dialog box.