settingseditor

### DccSnap

This registry entry determines whether the "Snap Point" option is used when creating a Surface Point or Vector Point auto feature. When this registry entry is set to TRUE (1), the measured values "snap to" the theoretical vector when a supported feature is measured. All the deviation is along the vector of the point. This is useful for focusing on a deviation along one particular vector.

Entry Name: DccSnap

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). The default value is 0.

For more information, see the "Snap List" topic in the "Creating Auto Features" in the PC-DMIS Core documentation.