core

### Option 3

Type a TIP/ command in the Edit window. Once you finish editing the vector, PC-DMIS calculates the best AB combinations that put the tip shank parallel to that vector.

The Auto Wrist Toggle icon in the Measurement Properties area in the Auto Feature dialog box is available if your measurement routine has a wrist probe. You can use this icon to enable PC-DMIS to determine the best wrist position to use when an Auto Feature is measured. For more information, see "Auto Wrist Toggle".