portable

## Calibrating a Romer Hard Probe

Accomplish the calibration of a Romer Infinite probe via the WinRDS software. PC-DMIS interfaces with WinRDS to acquire probe calibration data. Follow the steps found in the Arm Utilities User Guide document to calibrate your probe.

Use the PC-DMIS Probe Utilities dialog box to calibrate Perceptron Contour sensors. For information on how to calibrate Perceptron Contour sensors, see the "Calibrating a Perceptron Contour Sensor" topic.