core

### Local Temperature Settings

When it opens a measurement routine containing a TEMPCOMP command, PC-DMIS verifies the part sensor number with the local settings.

- If the values differ, PC-DMIS automatically updates the command to reflect the current settings, and a comment is inserted into the measurement routine reflecting the old and new values.

- If no local setting is available for the part sensor, PC-DMIS marks the TEMPCOMP command RED in the Edit window.