planner

#### Importing a Parasolid File

To import a Parasolid file:

1. Open the measurement routine in Planner into which you are going to import the Parasolid file. Your LMS license or portlock must be programmed with the Parasolid option.

2. Select File | Import | Parasolid. An Import dialog box appears.

3. Use the Import dialog box, and navigate to the folder that contains the file to import. Then select the file.

4. Click the Import button. Planner imports the CAD file. A progress bar appears and indicates its progress.

During the import process, you can cancel or stop the import.

- Cancel - This button cancels the import altogether. If you already had a CAD model loaded before the import, PC-DMIS retains the previous CAD model.

- Stop - This button stops the import, but keeps any imported CAD elements up to that point.