miim

### MLB-191 Came off surface

The analog probe is under-deflected during a scan move command.

As a result, SMP is put into Manual mode when:

- TrapScanDeflectStatus = False (System Default). The command is temporarily halted until SMP is put into automatic mode.

- TrapScanDeflectStatus = True. The command is not executed. The variable ScanDeflectStatus equals 0.

What you should do:

1. Check the part surface.

2. Check the current soft probe deflection value.

3. Initiate a user-generated scan error recovery routine.