settingseditor

### ConeAngleForMoveOverPath

The value for this registry entry is the half angle of a cone around the probe tip that determines how to move to avoid a collision. If the path direction at the point of a collision is within this cone of the tip vector, then a clearance move along the mount vector (arm vector) is attempted to avoid the collision. Otherwise, a clearance move along the tip vector is attempted.

Entry Name: ConeAngleForMoveOverPath

Entry Type: Real Number to specify angle in degrees. The default value is 35.