core

Step 1 - Select the ACR3 Probe Changer

To select the ACR3 Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer).

2. In the Probe changer type list, select ACR3:

Probe Changer dialog box - Type tab

3. To make this probe changer active and load the settings that are relevant to this probe changer, click Apply. Other tabs become visible after you click Apply.

4. In the Number of probe changers box, type the number of different types of probe changers.

5. In the Active probe changer list, select the item that represents the probe changer you are defining. If this is the first probe changer, it appears as Probe Changer 1 : TYPE=None.

6. Type the docking speed in the Docking speed box. The default value of 5% is appropriate for most machine configurations.

In the next step, you define the location of the probe body when you use the probe changer to switch probe components.