miim

## Testing the Lights in a Terminal

To test the lights in a terminal:

1. Download Tera Term from http://ttssh2.sourceforge.jp/index.html.en. Tera Term is an open-source free software terminal emulator.

2. Run Tera Term.

3. In Tera Term, create a new serial connection.

4. To set up the terminal, set the terminal transmit type for a new-line to be carriage return plus line feed (CR+LF). For help, refer to the Tera Term documentation.

5. Send a command and watch for a response. The response depends on the type of system: PWM or non-PWM.

PWM System

If you have a PWM system:

- To turn on the red light, type q.

- To turn on the green light, type e.

The following picture shows an example of a response:

For a complete list of keyboard keys for a PWM system, see "PWM Protocol".

Non-PWM System

If you have a non-PWM system:

- To turn on the red light, type 1.

- To turn on the green light, type 3.

The following picture shows an example of a response:

For a complete list of keyboard keys for a non-PWM system, see "Non-PWM Protocol".