Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
SetBoundaryConditionParams Method
See Also Send Topic Feedback | See Object Hierarchy Chart

nCrossings
  Required Long that sets the number of crossings for this boundary condition.

dRadius
  Required Double that sets the radius of the boundary condition.

dHalfAngle
  Required Double that sets the half-angle of the cone-type boundary condition, or is ignored if the boundary condition is not of cone type.

PCDLRN ActiveX DLL > BasicScan Object : SetBoundaryConditionParams Method

Glossary Item Box

# Description

Boolean value. Boolean returns true if the function succeeds, false if it fails.

# Syntax

Visual Basic
    Public Function SetBoundaryConditionParams( _
       ByVal nCrossings As Long, _
       ByVal dRadius As Double, _
       ByVal dHalfAngle As Double _
    ) As Boolean

# Parameters

nCrossings
  Required Long that sets the number of crossings for this boundary condition.
dRadius
  Required Double that sets the radius of the boundary condition.
dHalfAngle
  Required Double that sets the half-angle of the cone-type boundary condition, or is ignored if the boundary condition is not of cone type.

# Remarks

Boundary Condition | SetBoundaryConditionParams (nCrossings, dRadius, dHalfAngle)
--- | ---
Plane | Ncrossings
Cone | NCrossings,, dHalfAngle
Cylinder | NCrossings, dRadius
Sphere | NCrossings, dRadius

# See Also

BasicScan Object | BasicScan Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.