settingseditor

### DCCMode

Defines the Calibration method to use during Dual Arm calibration. When this registry entry is set to TRUE (1), PC-DMIS uses DCC mode. This allows you to supply the sphere positions and it does all the motion under computer control. When this value is set to FALSE (0), PC-DMIS prompts you to measure each sphere position using the CMM's jog box. Once you have taken the first hit on the top of the sphere, PC-DMIS takes the rest of hits in DCC mode.

Entry Name: DCCMode

Entry Type: Whole Number specifying DCC (1) or MANUAL (0). The default value is 0.