miim

### MP-515 IEEE 488 initialization failure

On an MP-30 system, there is an IEEE addressing or transmission error. There is a faulty IEEE chip or control board. It has failed to:

· Set up a talk address or a listen address, or

· Put the chip in talker-only, listener-only, talker-active, or listener-active modes.

For more information, see "MP Error Codes".

You should contact your Giddings & Lewis service representative.