miim

## LK Direct

TNT and PCiia card settings

GPIB0

Bus Timing 500ns

Cable length for high speed disabled

Primary Address 30

Secondary Address None

Terminate read on EOS No

Set EOI with EOS on write No

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 10

System Controller Yes

I/O Timeout 10 sec

Parallel Poll duration default

Enable Auto Serial Poll No

Enable CIC Protocol No

Assert REN when SC No

CUPE0

Primary Address 7

Secondary Address None

Terminate read on EOS No

Set EOI with EOS on write No

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 10

I/O Timeout 10 secs

Serial Poll Timeout 1 sec

Enable Repeat Addressing no