miim

### Probe Changer Support

For more information on how to use and configure the following probe changers, see the "Probe Changers" chapter.

ZEISSTC1

The ZEISSTC1 probe changer is usually used on machines with the ST2 or ST3 switching probe head. It is not used on machines with a scanning probe head. You must define the probe changer type as ZEISSTC1.

#### ZEISSTC2

The Zeiss GPIB/RS-232 Direct interface does not support the ZEISSTC2 probe changer.

#### DSE Head

This probe changer is used with the DSE rotating head. Define it as ZEISSTC_DSE.

#### RDS Head

This probe changer is used with the RDS rotating head. Define it as ZEISSTC_RDS.