miim

## Zeiss GPIB

GPIB0

Bus Timing 500ns

Cable length for high speed disabled

Primary Address 0

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write Yes

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 10

System Controller Yes

I/O Timeout 10 sec

Parallel Poll duration default

Enable Auto Serial Poll No

Enable CIC Protocol No

Assert REN when SC No

ZEISS0

Primary Address 8

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write Yes

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 3

I/O Timeout 10 secs

Serial Poll Timeout 1 sec

Enable Repeat Addressing No

ZEISS1

Primary Address 9

Secondary Address None

Terminate read on EOS Yes

Set EOI with EOS on write Yes

8 bit EOS compare No

Send EOI at end of write Yes

EOS byte 10

I/O Timeout 10 secs

Serial Poll Timeout 1 sec

Enable Repeat Addressing No