Collapse All Expand All

PC-DMIS 2019 R1 Object Library |
SetShankVector Method
See Also Send Topic Feedback | See Object Hierarchy Chart

I
  Required Long used to set the I component of the shank vector.

J
  Required Long used to set the J component of the shank vector.

K
  Required Long used to set the K component of the shank vector.

PCDLRN ActiveX DLL > ActiveTip Object : SetShankVector Method

Glossary Item Box

# Description

Sets the shank vector of the tip

# Syntax

Visual Basic
    Public Function SetShankVector( _
       ByVal I As Double, _
       ByVal J As Double, _
       ByVal K As Double _
    ) As Boolean

# Parameters

I
  Required Long used to set the I component of the shank vector.
J
  Required Long used to set the J component of the shank vector.
K
  Required Long used to set the K component of the shank vector.

# Return Type

Boolean value representing whether the call successfully set the shank vector values.

# See Also

ActiveTip Object | ActiveTip Members

Copyright © 2019. Hexagon Manufacturing Intelligence – Metrology Software, Inc. All Rights Reserved.