miim

### MLB-190 Too much probe deflection

The analog probe is over-deflected during a scan move command.

As a result, SMP is put into Manual mode when:

- TrapScanDeflectStatus = False (System Default). The command is temporarily halted until SMP is put into automatic mode.

- TrapScanDeflectStatus = True. The command is not executed. The variable, ScanDeflectStatus, equals 2.

What you should do:

1. Check the part surface.

2. Check the current soft probe deflection value.

3. Initiate a user-generated scan error recovery routine.