core

#### Calibrating the LSPX1SF / HR-X (HR-X1-SF) Probe Changer

The calibration process for the LSPX1SF / HR-X (HR-X1-SF) Probe Changer represents the steps that you would take to prepare for using any of the probe changers that PC-DMIS supports. The process discussed here is specific to the LSPX1SF / HR-X (HR-X1-SF) Probe Changer.

No inserts or extensions are used for any of the port positions.

Leitz LSPX1SF / HR-X (HR-X1-SF) rack

The LSPX1SF / HR-X (HR-X1-SF) stylus changer DOES NOT need to be mounted on the machine table parallel to either the X or Y axis. However, it must be oriented at an angle which matches an available wrist angle for loading and unloading. For mounting instructions, consult the documentation that came with your probe changer.

To calibrate your probe changer:

Step 1 - Select the LSPX1SF / HR-X (HR-X1-SF) Probe Changer

Step 2 - Define the Mount Point

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take the First Manual Hit

Step 6 - Take the Second Manual Hit

Step 7 - Take Manual Hits on the Top of Each Port

Step 8 - Review the Calibration Results

Step 9 - Recalibrate Individual Ports