miim

### Additional Notes

Use the Reflex interface with a Reflex controller on a manual Gage 2000 machine. You must set the Reflex box to Pass Through mode.

There are two "smart cards" inserted in the controller. The upper storage card is where the controller saves measurement routines. When you turn on the Reflex controller, the controller displays these screens:

- Copyright screen

- Language screen

- VolComp screen

- Home screen

To start the service:

1. Click Service Utilities.

2. Perform the probe qualification until you arrive at the Startup Options screen.

3. Select Pass Through mode.

Before you start PC-DMIS, rename the Reflex.dll to interfac.dll.

The Machine Options dialog box (Edit | Preferences | Machine Interface Setup) has these tabs for the Reflex interface:

Controller tab

See the "Setting the Communication Protocol" topic in the PC-DMIS Core documentation. The default values are:

- Comm Port 1

- 9600 Baud

- No parity

- 8 data bits

- 1 stop bit.

Axis tab

See the "Assigning the Machine Axes" topic in the PC-DMIS Core documentation.

Debug tab

See "Generating a Debug File".