core

#### CMM Acceleration

The CMM Acceleration area of the Acceleration tab allows you to change the maximum acceleration (at mm/sec2) along the X, Y, or Z axis of the CMM. Available options are:

Maximum X Axis Acceleration
The number in this box represents the maximum acceleration that the CMM will take when traveling along the X axis.

Maximum Y Axis Acceleration
The number in this box represents the maximum acceleration that the CMM will take when traveling along the Y axis.

Maximum Z Axis Acceleration
The number in this box represents the maximum acceleration that the CMM will take when traveling along the Z axis.