laser

#### Slot Command Mode Text

The Slot command inside the Edit window’s Command Mode looks like this:

SLT1 =FEAT/LASER/SQUARE SLOT,CARTESIAN

THEO/<1.895,1.91,1>,<0,0,1>,<0,1,0>,3,7

ACTL/<1.895,1.91,1>,<0,0,1>,<0,1,0>,3,7

TARG/<1.895,1.91,1>,<0,0,1>

DEPTH=3

SHOW FEATURE PARAMETERS=YES

SURFACE=THEO_THICKNESS,1

MEASURE MODE=NOMINALS

RMEAS=NONE,NONE,NONE

AUTO WRIST=NO

GRAPHICAL ANALYSIS=NO

FEATURE LOCATOR=NO,NO,""

SHOW_LASER_PARAMETERS=YES

POINT CLOUD ID=DISABLED

SENSOR FREQUENCY=25,OVERSCAN=2,EXPOSURE=18

FILTER=NONE