miim

## SP600 (SCR600 rack)

This probe changer requires no RS-232 communications port.

You can modify the following registry entries in the USER_Option section of the PC-DMIS Settings Editor:

- TCFinalAdjustDepthSP600 - This offset value provides the depth distance that is applied to a calibrated port location of your SP600 probe changer.

This value adjusts the port location forward or backward relative to the probe changer if you are directly in front of it.

A negative value adjusts the calibrated port location toward the front of the probe changer by the given distance.

A positive value adjusts the calibrated port location toward the back of the probe changer by the given distance.

- TCFinalAdjustHeightSP600 - This offset value provides the height distance that is applied to a calibrated port location of your SP600 probe changer.

This value adjusts the port location up or down relative to the probe changer if you are directly in front of it.

A negative value adjusts the calibrated port location up by the given distance.

A positive value adjusts the calibrated port location down by the given distance.

- TCFinalAdjustLengthSP600 - This offset value provides the length distance that is applied to a calibrated port location of your SP600 probe changer.

This value adjusts the port location forward or backward relative to the probe changer if you are directly in front of it.

A negative value adjusts the calibrated port location to the left by the given distance.

A positive value adjusts the calibrated port location to the right by the given distance.

Since probe changers can be placed on the machine in varying orientations with respect to the machine's axes, adjustments made to the calibration are relevant to the probe changer's own coordinates and not the machine's axes

Older Versions of PC-DMIS

For older versions of PC-DMIS (version 2.X), you must add the following to the PCDLRN.INI file under the [Option] title:

- ToolChanger=1

- ToolChangerType=SP600