planner

## Adding Dimensions to Features

In addition to selecting what features to measure, you also need to add dimensions to those features in your inspection plan so that when the associated measurement routine is generated and executed, information appears in the report for evaluation.

Planner supports some simple dimensions as well as the standard Feature Control Frame (FCF) dimensions. The simple dimensions below contain three relational dimensions (Angle, Distance, and Location) and the key-in dimension. These dimensions do not use FCFs to display their information. For information on working with these simple dimensions, see the Using Simple Relational Dimensions topic:

Angle Between

Distance

Location

Keyin

Planner also supports FCF dimensions. The standard FCF dimensions are organized by the following types. For information on working with FCF dimensions, see the Using Feature Control Frames topic:

Form

Straightness

Flatness

Circularity

Cylindricity

Orientation

Parallelism

Perpendicularity

Angularity

Location

Position

Concentricity

Coaxiality

Symmetry

Profile

Line Profile

Surface Profile

Runout

Circular Runout

Total Runout

More:

Using Simple Relational Dimensions

Using Feature Control Frames