core

Step 6 - Take the Second Manual Hit

For the SCP600 Probe Changer, you will take the second manual hit in the Z direction, on the horizontal face on top of the rack to the left of the open port.

The prompt for the second hit on the top is:

PC-DMIS Message

Please take a hit on the black top face on the left side of port 1.

The hit should be on the left portion and not inside a recessed circle.

After completing this hit, DCC calibration will beging to complete the measurement of this port.

Use your machine's jog box to measure the second hit on the top, flat, plastic surface of the port, left of the opening:

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

In the next step, you review the calibration results.