core

### LKDriver Interface

The LKDriver interface is used with an LK machine with a LK3000 or LK2000 controller. You must obtain the common driver software directly from LK. You must install and configure it before you attempt to install and use the PC-DMIS interface that utilizes it.

The common driver DLL is named something similar to LKCMMDRV53.DLL depending on the version number of the driver. There are also various other DLL’s that LK provides with the driver that must be present for the driver to work properly. The earliest version that you can use with the PC-DMIS interface is LKCMM21.DLL. Earlier versions are not compatible.

Before you start PC-DMIS, rename lkdriver.dll to interfac.dll.

The Machine Options dialog box (Edit | Preferences | Machine Interface Setup) has three tabs for the LKDriver interface:

LK Driver tab

See the "LK Driver tab" topic.

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).

You can access the MIIM help file from this link: .