core

#### Calibrating the Travel Rack HR-X1-TR

The calibration process discussed in this section is specific to the Travel Rack HR-X1-TR.

The probe changer mounts onto the drive leg of the CMM. For mounting instructions, consult the documentation that came with your Travel Rack HR-X1-TR.

Mounted Travel Rack HR-X1-TR

The probe changer travels with the moving portal of the machine. The stylus change is done horizontally. Therefore, the TESASTAR-M brings the sensor into the right position.

Since the change rack moves with the portal, there are no additional travelling distances to perform a change of configuration, as would be the case with a standard rack. This enables quick changes of the styli configuration anywhere in the measurement volume.

To calibrate your probe changer:

Step 1 - Select the Travel Rack HR-X1-TR

Step 2 - Define the Mount Point

Step 3 - Define the Number of Ports

Step 4 - Prepare for Calibration

Step 5 - Take the Manual Hits