miim

### Interface-Specific Options

The following registry entries are available for the Leica interface.

- TrackerIPAddress = 192.168.0.1

- TrackerPort = 700

- RequestInterval = 300 - Specifies how frequently readouts are updated, in milliseconds.

- ScanInterval = 100 - Specifies how frequently samples are taken in scanning, in milliseconds.

- AImToNextPoint = TRUE - Specifies whether to automatically aim the tracker to the first point of a feature after taking a hit in DCC mode.

- Vector Distance - Is the distance for the pulled-away vector.

- WeatherMonitor - If you do not use a weather monitor, set the value to 0. To read and automatically set refraction, set the value to 2.

- HasNivel - If there is a nivel, set the value to 1. Otherwise, set it to 0.

- HasCamera - If there is a camera, set the value to 1. Otherwise set it to 0.

- NivelXTilt - Is the current X tilt of the nivel. Do NOT set this manually. The software sets it after it performs an orient-to-gravity.

- NivelYTilt - Is the current Y tilt of the nivel. Do NOT set this manually. The software sets it after it performs an orient-to-gravity.

- NivelXTolerance - Specifies the X tolerance to warn the user that the system is not leveled.

- NivelYTolerance - Specifies the Y tolerance to warn the user that the system is not leveled.

- SecondsToCheckEnvironment - Specifies how often the weather monitor is to be read, in seconds.

- SecondsToCheckGravity - Specifies how often the nivel is to be read, in seconds.

- DelayToStartSendingScanPointsToManualHit - Specifies the number of milliseconds that the user needs to press the Take-Hit button before automatic feature scanning occurs.