miim

# MIIM Overview

MIIM stands for Machine Interface Installation Manual. The MIIM documentation gives instructions and settings for the different supported machine interfaces:

CMM

Brown & Sharpe Excel (Sharpe) Interface

CMM-OS Interface

DEA – RS232 INTERFACE

FDC Interface

I++ DME Client Interface

Johansson Interface

Leitz-Common Firmware Interface

LK Direct Serial/GPIB Interface

LK Direct TCP Interface Installation

LK Driver

Manual CMM Interface

Mitutoyo Manual-GPIB Interface

Mora Interface

Reflex Interface

Sheffield Interface

Wenzel Interface

Zeiss GPIB/RS-232 Direct Interface

Zeiss-IP UDP/TCP Direct Interface

Portable

Faro Arm Interface

Faro Tracker Interface (SMX)

Leica Interface

Romer/CIMCORE WINRDS Interface

Vision

FDC-SLC Interface

FDC-VisionBox Interface

HP-C-Ve

METRONICS QC5000 INTERFACE (HEIDENHAIN IK5000)

PC-DMIS Micro-Vu Interface Installation Notes

Mycrona DCC

Miscellaneous References

Common Settings

Common Settings for Vision or Multi-Sensor Machine Interfaces

External Probe Head

External Rotary Table

GPIB Settings

I++ DME Server Setup

Notification Center Interface

PC-DMIS Vision Frame Grabber and Camera Setup

Tool Changers

Valisys Mode

Volumetric Compensation

Changes to your machine's interface settings can adversely affect your measurement machine's behavior. You should only make changes to the interface settings if you understand the ramifications or if Hexagon Technical Support instructs you to do so.