planner

Step 5 - Take a Point with the Over-Hang of the Collet

For the LSPX5 / HR-XS Probe Changer, the prompt to take a point on the over-hang of the collet is:

PC-DMIS Message

Please take a point on top of the clamp for port 1 using the over-hang of the collet near the probe pin

Prompt to take a point with the over-hang of the collet

You must take a point on the top of the first port using the over-hang of the collet. The image below shows the over-hang of the collet:

Over-hang of the collet

The image below shows how to take a point with the over-hang:

One point with the over-hang of the collet

In the next step, you define the location of the first port.