planner

#### Remove Outliers / Standard Deviation Multiple

For a Best Fit (BF) or Best Fit Recompensate (BFRE) plane, you can choose to remove outliers based on the distance from the best fit feature. This allows the removal of anomalies that arise in the measurement process.

Planner first fits a plane to the data and then determines which points are outliers based on the standard deviation multiple. It then does the following:

1. Recalculates the best fit plane with those outliers removed.

2. Checks for outliers again.

3. Recalculates the best fit plane.

4. Continues to repeat this process until no more outliers exist or until Planner cannot compute the plane. (Planner can't compute the plane if there are fewer than three data points.)