settingseditor

### Dimension132Columns

This option controls the printing format of feature locations in the inspection report. When this registry entry is set to TRUE (1), PC-DMIS prints all feature locations in a 132 column format.

Entry Name: Dimension132Columns

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). The default value is 0.

The following list describes the columns in the 132 column printout format:

Column 1 to 10: X nominal
Column 11 to 20: X measured
Column 21 to 28: X deviation
Column 31 to 40: Y nominal
Column 41 to 50: Y measured
Column 51 to 58: Y deviation
Column 61 to 70: Z nominal
Column 71 to 80: Z measured
Column 81 to 88: Z deviation
Column 91 to 100: T error (normal to surface error)
Column 101 to 101: Out of Tol flag "*"
Column 104 to 105: Feature type
Column 108 to 117: Feature ID
Column 118 to 127: Measured Diameter if any