settingseditor

### ConnectionTypeArm(1-4)

Specifies the connection type for the given arm (1-4) arm to the current (master) computer. Values can be provided for Arm 1-4 respectively. This value is only used this is the Master computer set with a value of 1 for Mode.

Entry Name: ConnectionTypeArm(1-4)

Entry Type: Whole Number specifying 0 (Direct Connection) or 1 (Remote Connection). The default value is 1.