core

### TEMPCOMP/ORIGIN Command in the Edit Window

When you click the OK button to accept the inputs in the Temperature Compensation Setup, PC-DMIS inserts a TEMPCOMP/ORIGIN command into the measurement routine. Here is the same command in both Edit window modes:

Command Mode

Summary Mode

Normally, a measurement routine only uses one TEMPCOMP command. The TEMPCOMP command should be placed near the top of the measurement routine prior to any measurements. When you execute the measurement routine, it executes according to the various input parameters.