settingseditor

### ColmapLowTol

This registry entry provides the default lower tolerance value that appears in the Pointcloud Operator dialog box for a POINT COLORMAP or FACE COLORMAP operator.

Entry Name: ColmapLowTol

Entry Type: Real Number that specifies the lower tolerance in mm. The default value is -1.

See the "SURFACE COLORMAP" or "POINT COLORMAP" topic of the PC-DMIS Laser help file for more information.