core

#### Temperature compensation enabled check box

The Temperature compensation enabled check box tells PC-DMIS to use temperature compensation.

- If cleared, PC-DMIS does not perform any temperature compensation, and the TEMPCOMP command (if present in the measurement routine) has no effect.

- If marked, PC-DMIS behaves according to the input parameters.

If you mark this check box and choose one of the compensation methods where PC-DMIS does the part compensation rather than the machine controller, the diameter for probes on non-portable machines in the Edit Probe Data dialog box may vary with the current part temperature. See "Edit Probe Data" in the "Defining Hardware" chapter.