nc

### PC-DMIS NCI Differences

The following are fundamental differences of PC-DMIS NCI.

Differences from PC-DMIS:

- DCC only.

- Calibration Tool Location is definable for DCC probe calibration.

- Initial rough location of the part must be specified in Machine Coordinates (no manual teach-in).

Differences from PC-DMIS NC:

- No export of a measurement path measurement routine (.cnc).

- The active work offset has no effect. All motion is generated in machine coordinates and adjusted to match the active work offset.

- Only one machine is defined using the NC Gateway server application. The machine must have Machine ID = 1.