miim

# Common System Options

· AxisX=0

· AxisY=2

· AxisZ=4 - These options allow you to reassign machine axis in PC-DMIS. The default shown gives X=X, Y=Y, and Z=Z. The value of each machine axis is defined as follows: X=0, -X=1, Y=2, -Y=3, Z=4, -Z=5. For example, if the -X machine axis to is be read as +X in PC-DMIS then you would define AxisX=1. Likewise, if you want the machine -Z axis to be read as +Y then you would define AxisY=5.
WARNING: the axis directions you define MUST form a right-handed coordinate system.

· DebugLog=FALSE If set to TRUE this option turns on debugging reporting. It sends messages to the debug file that are helpful in determining problems with the interface.

· DebugFile=debug.txt This option specifies the file that all debug information will be sent to.

· DebugPosReport=0 N/A

· DebugToCMM=3 N/A

· DebugFromCMM=3 N/A

· DebugWindow=FALSE This option sends debug reporting directly to a window on the screen.

· DebugTitle=Interface N/A