miim

### Machine Axis Limits

PC-DMIS will retrieve the min and max values for the X, Y and Z axes from the driver configuration and perform software tests for the validity of commanded moves. For these tests to be meaningful you should make sure that reasonable values are stored in the common driver configuration.

The tests can essentially be disabled by storing large positive values for the maximums and large negative values for the minimums.