core

Step 6 - Take the Second Manual Hit

You will take the second hit for the HR-MS (used with LSPX1) Probe Changer on the front surface of the left side of the second port.

Once the first manual hit is completed, the following message box appears:

PC-DMIS Message

Take a hit on the front surface of the left side of port 2.
It should be taken near the top and
near the side but avoid any tapered corner.

1. When you are ready to take the second measurement, click OK.

2. Use your machine's jog box to take the second manual hit on the front surface of the left side of port 2. Take the hit near the top and side on the flat surface of the port (avoid the tapered corner).

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

In the next step, you take the third manual hit.