core

#### Setting Boundary Points Using the Measured Point Method

To set the boundary of the scan using measured points, touch the probe on the part. This automatically updates the value of the boundary point that is currently selected in the Boundary list. The focus then moves to the next boundary point (if there are any in the list).

In the case of a PATCH scan, an extra boundary point is added automatically if the current point is the last point in the list. The PATCH scan displays the last point (this is the same as the previous point). PC-DMIS deletes this last point when you select the OK button in the scan dialog box (Insert | Scan).