miim

## Procedure to Copy Mechanical Offset Values from Sheffield Key to USER_Sheffield Key

To copy the mechanical offset values from the Sheffield key to the USER_Sheffield key:

1. Open the Registry Editor.

2. Navigate to the USER_Sheffield key:

My Computer\HKEY_LOCAL_MACHINE\SOFTWARE\WAI\PC-Dmis\USER_Sheffield

3. Right-click the right-side pane.

4. Select New | String Value.

5. Rename the ‘New Value #1’ to MechanicalOffsetX.

6. Repeat steps 3 to 5 for values MechanicalOffsetY and MechanicalOffsetZ.

7. Navigate to the Sheffield key:

My Computer\HKEY_LOCAL_MACHINE\SOFTWARE\WAI\PC-Dmis\Sheffield

8. Double-click the MechanicalOffsetX value in the right pane

9. Press Ctrl + C to copy the value.

10. Navigate to the USER_Sheffield key:

My Computer\HKEY_LOCAL_MACHINE\SOFTWARE\WAI\PC-Dmis\USER_Sheffield

11. Double-click the MechanicalOffsetX value/

12. Press Ctrl + V to paste the value.

13. Repeat steps 7 to 12 for values MechanicalOffsetY and MechanicalOffsetZ.

14. Close the Registry Editor.