portable

## Working with the MI.Probe

MI.Probe Button Assignments

A - Trigger button

B - LED display

C - Thumb buttons

MI.Probe details

Button | Action | Function
Trigger button | Press | Triggers a single measurement, starts and stops scanning.
Left Thumb button | Press less than one second | Deletes the last probed point.
Left Thumb button | Press longer than one second | No action.
Right Thumb button | Press less than one second | Finishes geometry measurements (for example, when completing the last probed point for a plane measurement).
Right Thumb button | Press longer than one second | Switches between Single and Scan modes.
Right and Left Thumb button | Press simultaneously | Activates the unit when in Sleep mode.
Trigger button | Press for six seconds until middle LED turns off, then let go and press until middle LED turns on. | Reboots the unit.
Trigger button | Press and hold for six seconds until the middle LED turns off. | Switches the unit off if it is on.
Trigger button | Press and hold for two seconds until the middle LED turns on. | Switches the unit if it is off.

MI.Probe LED Display

LED | Color | Status
Left | Red | The last measurement was not successful.
Left | Green | The last measurement was successful.
Left | Red and Green | -
Left | Off | The probe is not ready for measuring.
Middle | Blue | The probe is active and the serial communication via Bluetooth is established.
Middle | Red | The probe is active but there is no serial communication via Bluetooth.
Middle | Blue and Red (one is flashing) | The battery is low.
Middle | Off | The probe is switched off or is in Standby mode.
Right | White | Scan mode is active but scanning has not started.
Right | Red | -
Right | White and Red | Scan mode is active and scanning is in progress.
Right | Off | Single mode is active.

More:

Measuring with the MI.Probe