core

Step 5 - Take the First Manual Hit

For the SCP600 Probe Changer, a series of message boxes prompts you through the process of measuring two manual hits. Two hits are required to define the location of this rack in the machine’s workspace. Follow the prompts and take the needed hits as shown in the pictures for each hit.

You will take the first manual hit in the XY plane on the vertical face in front of the rack on the left side of the port. The prompt is:

PC-DMIS Message

Please take a hit on the black front face on the left side of port 1.

Prompt for the first manual hit

Use your machine's jog box to measure the first hit on the front face to the port, to the left of the opening:

In the next step, you take the second manual hit.