cmm

### Adaptive Cylinder Line Scan Strategy

The Adaptive Cylinder Line Scan strategy for the Cylinder Auto Feature scans a number of lines along the cylinder parallel to its axis. The cylinder can be a threaded surface or a smooth surface.

When you use this strategy, the diameter of the probe tip must exceed the size of the valleys in-between the threads in order to prevent probe shanking.

The strategy's tabs are located in the Probe Toolbox in the Auto Feature dialog box (Insert | Feature | Auto | Cylinder):

- Setup tab

- Filters tab

- Advanced tab

For complete information about the Probe Toolbox and selecting a measurement strategy, see "Working with Measurement Strategies".