planner

Step 1 - Select the LSPX5 / HR-XS Probe Changer

To select the LSPX5 / HR-XS Probe Changer:

1. Select the Type tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer).

2. In the Probe changer type list, select LSPX5 / HR-XS:

Probe Changer dialog box - Type tab

3. To make this probe changer active and load the settings that are relevant to this probe changer, click Apply. Other tabs become visible after you click Apply.

4. In the Number of probe changers box, specify the number of probe changers that you want to define.

5. In the Active probe changer list, select the list item that represents the probe changer that you want to define. If this is the first probe changer, it appears as Probe Changer 1: TYPE=None.

In the next step, you define the mount point.